|  |
| --- |
| A picture containing indoor, pan, water basin  Description automatically generated |
| **ESP32 DIY IOT Development Kits** |
| **User Manual** |

Abstract

User Manual describing the ESP32 DIY IOT Development Kits. Kits features, content and project ideas provided.

|  |  |
| --- | --- |
| IBT-QESP32-COR-X-UM | Icon  Description automatically generated |
|  |
| www.iot-bots.com |

Table of Contents

[Revision History 2](#_Toc59910038)

[Overview 3](#_Toc59910039)

[Features 3](#_Toc59910040)

[Description 3](#_Toc59910041)

[qBox AMC Enclosure Kit (No SMA) 4](#_Toc59910042)

[qBox AMC Enclosure Kit (One SMA) 5](#_Toc59910043)

[qBox AMC Enclosure Kit (Two SMAs) 6](#_Toc59910044)

[qBox AMC Enclosure Kit parts 6](#_Toc59910045)

[Specification 13](#_Toc59910046)

[qBox AMC Enclosure Kit content 13](#_Toc59910047)

[Project ideas 14](#_Toc59910048)

[Abbreviations 15](#_Toc59910049)

[Trademark notice 15](#_Toc59910050)

[Ordering info 15](#_Toc59910051)

# Revision History

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **№№** | **Version** | **Date** | **Author** | **Description** |
| 1 | 1.0 | 02.01.2020 | Iotbotscom | Initial |
| 2 |  |  |  |  |
| 3 |  |  |  |  |

# Overview

Perfect for any DIY IOT project, qBox AMC Enclosure Kit series is the part of the newest HW platform designed to help hobbyists, makers and all DIYers to build environmental ready IOT solutions.

# Features

* Flanged IP65 waterproof enclosure: Sealed, made of high-quality ABS material suitable for indoor and outdoor DIY IOT projects;
* Incorporated PG7 cable glands: Two cable inputs securely allow bringing the power in and connecting sensors and actuators;
* Perfect fit PCB: High-quality double-sided PCB with 0.1" hole spacing for DIP integrated circuits, modules, and main controller board;
* Dedicated placement for controller board: Well-designed PCB allows to carry Arduino MKR Compatible MCU board;
* Built in SMA connectors: Up to two SMA Straight Female to IPEX（u.FL） adapter cables give external antennas connections to your wireless board;
* Rich connectors set installed: Four terminal blocks, Grove, 4-pin JST and 0.1" AMC compatible interface connectors.

# Description

qBox AMC Enclosure Kits are part of qBox AxC Enclosure Kits line. qBox AxC Enclosure Kits line is based on qBox Enclosure Kits product line and developed especially to be used with AFC or AMC boards. So, each kit PCB has dedicated connectors main CPU board could be plugged in (AFC or AMC).

Each qBox AMC Enclosure Kit consists of durable waterproof IP65 enclosure with installed PG7 glands, double sided PCB with connectors installed and integrated SMA to u.FL adapter cable (up to two, depending on kit model) and connectors set.

## qBox AMC Enclosure Kit (No SMA)

qBox AMC Enclosure Kit (No SMA) is the simplest member in qBox AMC Enclosure Kit family. It has no integrated SMA to u.FL adapter cable, but still able to keep wireless connectivity device with internal antennas.

|  |  |  |
| --- | --- | --- |
| A picture containing indoor, vessel, pan, water basin  Description automatically generated | A picture containing indoor, pan  Description automatically generated | |
| Pic.1. qBox AMC Enclosure Kit (No SMA) common view | | |
| A close up of a logo  Description automatically generated | |
| Pic. 2. qBox AMC Enclosure Kit (No SMA) dimensions | |

## qBox AMC Enclosure Kit (One SMA)

qBox AMC Enclosure Kit (One SMA) is the member of qBox AMC Enclosure Kit family which is able to bring up to one external antenna signal to IOT device located inside. It has one integrated SMA to u.FL adapter cable.

|  |  |  |
| --- | --- | --- |
| A picture containing indoor, pan, water basin  Description automatically generated | A picture containing indoor  Description automatically generated | |
| Pic.3. qBox AMC Enclosure Kit (One SMA) common view | | |
| A screenshot of a cell phone  Description automatically generated | |
| Pic. 4. qBox AMC Enclosure Kit (One SMA) dimensions | |

## qBox AMC Enclosure Kit (Two SMAs)

qBox AMC Enclosure Kit (Two SMA) is the most charged member of qBox AMC Enclosure Kit family which has got two integrated SMA to u.FL adapter cables.

|  |  |  |
| --- | --- | --- |
| A picture containing pan  Description automatically generated | A picture containing indoor  Description automatically generated | |
| Pic.5. qBox AMC Enclosure Kit (Two SMAs) common view | | |
| A close up of a map  Description automatically generated | |
| Pic. 6. qBox AMC Enclosure Kit (Two SMAs) dimensions | |

## qBox AMC Enclosure Kit parts

Each qBox AMC Enclosure Kit has got several parts built in.

|  |
| --- |
| A picture containing text, electronics  Description automatically generated |
| Pic.7. qBox AMC Enclosure Kit parts |

External DC voltage from power adapter or solar system could be brought by cable through the one gland inner and another gland gives opportunity to connect external sensors or actuators.

Up to two (depending on kit type) GSM / LTE / WiFi / LoRa / etc. external antennas could be connected to wireless board u.FL PCB connector via SMA to IPEX (u.FL) adapter cables glued into enclosure wall.

Two M3 self-tapping screws securely attach the PCB to the enclosure. Same time board could be easily removed.

Enclosure has enough room to keep with or without stacking header one IOT controller board like Arduino MKR Compatible (AMC), power supply (DC/DC), OLED display and sensor modules using plain grid proto holes.

|  |  |
| --- | --- |
|  | A picture containing electronics  Description automatically generated |
| Pic.8. qBox AMC Enclosure Kit with Arduino MKR Compatible (AMC) board installed | Pic.9. qBox AFC Enclosure Kit with Adafruit Feather Compatible (AFC) board installed |

Each board has got four pluggable 3,5mm terminal blocks, one Grove, one 4-pin JST and two low profile pass-through 0,1” SMT AMC interface compatible connectors installed. Several DIP 0.1" I2C and SPI interface connectors could be populated. Two separate power traces for VDD and GND along short PCB sides allow bring the power to sensor boards.

|  |
| --- |
| A picture containing text, circuit, electronics  Description automatically generated |
| Pic.10. qBox AMC Enclosure Kit PCB common view (Front and Back) |

Each AMC connector pin has got a trace with DIP contacts that wires from other modules could be easily soldering.

Connector list:

* X1: External power connection through pluggable 3,5mm terminal block;
* X2…X4: External Input / Output sensor / actuator connections through pluggable 3,5mm terminal blocks;
* X5, X6: IOT board connectors (low profile 0,1” pass through SMT receptacle);
* X7: I2C sensors connector placement (0,1” DIP) with pins: VDD, GND, SCL, SDA, IO;
* X8: OLED I2C connector placement (0,1” DIP) with pins: VDD, GND, SCL, SDA;
* X9: SPI sensors connector placement (0,1” DIP) with pins: VDD, GND, SCK, MISO, MOSI, CS, IO;
* X10: 4 pins JST I2C&Power connector with pins: VDD, GND, SCL, SDA;
* X11: 4 pins Grove compatible I2C&Power connector (2,0 mm SMT) with pins: VDD, GND, SCL, SDA.

|  |
| --- |
| Diagram, schematic  Description automatically generated |
| Pic.11. qBox AMC PCB Connectors |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| There are VDD, GND and I2C connections between appropriate connectors pins and CPU board, so no needs to make these connections separately, just plug a CPU board and I2C sensors to Grove or JST connectors and get solution working. Two separate power traces for VDD and GND along short PCB sides allow bring the power to sensor boards.   |  | | --- | | A picture containing text, electronics  Description automatically generated | | Pic.12. qBox AMC JST and Grove connectors pinout |  |  |  | | --- | --- | | A picture containing electronics, circuit  Description automatically generated |  | | Pic.13. Grove and JST sensors board connection examples | | |

|  |
| --- |
| A picture containing graphical user interface  Description automatically generated |
| Pic.14. AMC PCB Front Copper traces |

|  |
| --- |
| A picture containing text, electronics  Description automatically generated |
| Pic.15. AMC PCB Back Copper traces |

IOT board connector pins have power and main interfaces names printed out on PCB. The rest of the pins have conditional names as Jxx.

|  |  |
| --- | --- |
|  |  |
| Pic.16. qBox AMC Enclosure Kit PCB | |

Low profile 0,1” pass through SMT connectors allow to carry Controller board as closer as possible to Kit PCB, saving space above that board to place additional components, like battery, OLED or sensors.

|  |
| --- |
| A picture containing circuit, electronics  Description automatically generated |
| Pic.17. Low profile 0,1” pass through SMT connectors |

Transparent lid allows to see internal parts, electronics, LEDs and even display and is able to hold LiPol battery or battery holder to be applied to the internal surface.

|  |  |
| --- | --- |
| A close up of a machine  Description automatically generated | A close up of a camera  Description automatically generated |
| Pic. 18. 2xAAA battery holder apllied to a tranparent lid (assembled view) | Pic. 19. 2xAAA battery holder apllied to a tranparent lid (inside view) |

# Specification

Housing Material: ABS

Water and Dust Proof: IP65

Enclosure Outer Size: 5.42"x2.72"x1.99" (L\*W\*H)

Enclosure Inner Size: 3.69"x2.42"x1.7" (L\*W\*H)

Gland model: PG7

Cables with diameters: 0.12-0.25"

PCB size: 3.42"x2.37"

SMA u.FL adapter cables : up to 2

SMA u.FL adapter cable length : 3.15”

# qBox AMC Enclosure Kit content

* IP65 waterproof enclosure with two PG7 glands installed and up to two SMA u.FL adapter cables glued (depending on kit type);
* High quality prototyping double sided PCB mounted with two M3 self-tapping screws and connectors installed:
  + Arduino MKR Compatible board female headers set (two low profile pass-through 0,1” pitch 1x14 pins connectors);
  + Four 3,5mm 2 pins terminal blocks;
  + Grove 2mm connector;
  + 4-pin JST I2C&Power connector;
* Four 3,5mm 2 pins terminal plugs;
* Packaging bag and shipping box.

# Project ideas

Using qBox AMC Enclosure Kits the variety of IOT DIY and POC projects could be done, like LoRa-based soil moisture monitoring project, home WiFi garage door opener, NB-IOT beehive monitoring system, GSM GPS asset tracking solution and many others.

|  |  |
| --- | --- |
|  |  |
| Pic. 20. Arduino MKR Zero controller | Pic. 21. WiFi ESP32 Sensor Hub project |

|  |  |
| --- | --- |
| A close up of a device  Description automatically generated | A picture containing indoor, pan  Description automatically generated |
| Pic. 22. LTE GPS BG96 tracker with RS485 port (LLS sensor) | Pic. 23. Arduino MKR LoRa controller |

# Abbreviations

|  |  |  |
| --- | --- | --- |
| №№ | Abbreviation | Explanation |
| 1 | AFC | Adafruit Feather Compatible |
| 2 | AMC | Arduino MKR Compatible |

# Trademark notice

All referenced brands, product names, service names, and trademarks are the property of their respective owners.

# Ordering info

|  |  |  |
| --- | --- | --- |
| **№№** | **Item** | **SKU** |
| 1 | qBox AMC DIY IOT Enclosure Kit (No SMA) | IBT-QBX- AMC -0 |
| 2 | qBox AMC DIY IOT Enclosure Kit (One SMA) | IBT-QBX- AMC -1 |
| 3 | qBox AMC DIY IOT Enclosure Kit (Two SMAs) | IBT-QBX- AMC -2 |